# Help on 'UPS Status'

Status: Output Status of this UPS. Values: OK, Powerfail, Battery low, Bypass, no output, shutdown, sleep, etc. See your UPS manual.
Input Voltage: UNITS RMS Volts. The magnitude of the present input voltage.
Input Frequency: UNITS Hertz. The present input frequency.
Output Voltage: UNITS RMS Volts. The magnitude of the present output voltage.
Output Frequency: UNITS Hertz. The present output frequency.
Load: UNITS percent: The percentage of the UPS power capacity presently being used on this output line, i.e., the greater of the percent load of true power capacity and the percent load of VA.
Seconds on Battery: In case of UPS running on batteries, this counts the seconds since the dicharge began. If the unit is on battery power, the elapsed time since the UPS last switched to battery power, or the time since the network management subsystem was last restarted, whichever is less. Zero shall be returned if the unit is not on battery power.
Battery Capacity: UNITS percentage. Estimated chargelevel of the batteries.
Autonomy Time: UNITS minutes. An estimate of the time to battery charge depletion under the present load conditions if the utility power is off and remains off, or if it were to be lost and remain off.
Battery Temperature: UNITS degrees Centigrade. The ambient temperature at or near the UPS Battery casing.
Last test Result:
Battery Voltage: UNITS Volt DC.The magnitude of the present battery voltage.
For more information - see user manual of your CS121.