<div class="tt" id="enummod">
<script type="text/javascript">_dw("Check this box to list the modules per string.")</script><br>
<script type="text/javascript">_dw("Each string counts the modules from one upwards.")</script><br>
<script type="text/javascript">_dw("The alternative is to address all batteries in one sequence.")</script>
</div>
<div class="tt" id="eqboxTT">
<script type="text/javascript">_dw("Check this box to activate Equalizing.")</script>
</div>
<div class="tt" id="enumboxTT">
<script type="text/javascript">_dw("Check this box to switch the module ids to be displayed per string rather than in one total sequence.")</script>
</div>
<div class="tt" id="modtype">
<script type="text/javascript">_dw("Please choose the type of the connected BACS modules.")</script>
</div>
<div class="tt" id="modcnt">
<script type="text/javascript">_dw("Please enter the total number of BACS modules, that shall be monitored, here.")</script>
</div>
<div class="tt" id="strcnt">
<script type="text/javascript">_dw("Please enter the number of strings, in which the modules are arranged, here.")</script>
</div>
<div class="tt" id="batcap">
<script type="text/javascript">_dw("Please enter the capacity in Ampere of the battery type you use in this battery group, eg. If you have 64 batteries, each 24Ah, then enter '24' here.")</script>
</div>
<div class="tt" id="batvolt">
<script type="text/javascript">_dw("Please enter the Volt of the battery type you use in this battery group.")</script>
</div>
<div class="tt" id="minV">
<script type="text/javascript">_dw("This is the lowest measured voltage for a battery that does not trigger an alarm.")</script>
</div>
<div class="tt" id="maxV">
<script type="text/javascript">_dw("This is the highest measured voltage for a battery that does not trigger an alarm.")</script>
</div>
<div class="tt" id="minT">
<script type="text/javascript">_dw("This is the lowest measured temperature for a battery that does not trigger an alarm.")</script>
</div>
<div class="tt" id="maxT">
<script type="text/javascript">_dw("This is the highest measured temperature for a battery that does not trigger an alarm.")</script>
</div>
<div class="tt" id="minOhm">
<script type="text/javascript">_dw("Enter lower threshold for resistance warnings here.")</script>
</div>
<div class="tt" id="maxOhm">
<script type="text/javascript">_dw("Enter upper threshold for resistance warnings here.")</script>
</div>
<div class="tt" id="warnlevels">
<script type="text/javascript">_dw("Please enter the thresholds beyond which warnings should be generated.")</script>
</div>
<div class="tt" id="almlevels">
<script type="text/javascript">_dw("Please enter the thresholds beyond which alarms should be generated.")</script>
</div>
<div class="tt" id="minW">
<script type="text/javascript">_dw("Enter lower threshold for warnings in this column.")</script>
</div>
<div class="tt" id="maxW">
<script type="text/javascript">_dw("Enter upper threshold for warnings in this column.")</script>
</div>

<div class="tt" id="minV_w">
<script type="text/javascript">_dw("Enter lower threshold for voltage warnings here.")</script>
</div>
<div class="tt" id="maxV_w">
<script type="text/javascript">_dw("Enter upper threshold for voltage warnings here.")</script>
</div>
<div class="tt" id="minT_w">
<script type="text/javascript">_dw("Enter lower threshold for temperature warnings here.")</script>
</div>
<div class="tt" id="maxT_w">
<script type="text/javascript">_dw("Enter upper threshold for temperature warnings here.")</script>
</div>
<div class="tt" id="minOhm_w">
<script type="text/javascript">_dw("Enter lower threshold for resistance warnings here.")</script>
</div>
<div class="tt" id="maxOhm_w">
<script type="text/javascript">_dw("Enter upper threshold for resistance warnings here.")</script>
</div>
<div class="tt" id="eqrng">
<script type="text/javascript">_dw("Enter range within which equalizing should operate here.")</script>
</div>
<div class="tt" id="reinitBACS">
<script type="text/javascript">_dw("Press this button to restart the BACS bus communication now.")</script><br>
<script type="text/javascript">_dw("This will reset your BACS system and measure the impedance within the next 60 minutes 4 times to get a precise result. Additionally this button applies your changes to BACS configuration and restarts the BACS bus without the need for BACS reboot.")</script><br>
<script type="text/javascript">_dw("Remember you still need to SAVE & REBOOT to make your changes permanent.")</script>
</div>
<div class = "tt" id = "fVoltDiffThreshold">
<script type="text/javascript">_dw("Should the difference in voltage of a battery to the average voltage of all batteries exceed this threshold, an alarm can be raised.")</script>
</div>
<div class="tt" id="temperatureoffset">
<script type="text/javascript">_dw("Change BACS measurings to your reference thermometer.")</script><br>
<script type="text/javascript">_dw("Eg. By +2.0 you would add 2 &deg;C to the real BACS temperature measurings on all BACS modules.")</script><br>
<script type="text/javascript">_dw("A negative value would deduct this offset to all BACS modules and shows a 2 &deg;C lower temperature than the raw data.")</script><br>
<script type="text/javascript">_dw("Please note that such offsets should be noted in your battery reports.")</script>
</div>
<div class="tt" id="impedanceoffset">
<script type="text/javascript">_dw("Change BACS measurings to your reference RI measuring device.")</script><br>
<script type="text/javascript">_dw("Eg. By -2.2 you would deduct 2.2 mOhms from the real BACS RI measuring on all BACS modules.")</script><br>
<script type="text/javascript">_dw("A positive value would add this offset to all BACS modules and show a higher value than the BACS raw data.")</script><br>
<script type="text/javascript">_dw("Please note that such offsets should be noted in your battery reports.")</script>
</div>
<div class = "tt" id = "DischargeDetectionFlags">
<script type="text/javascript">_dw("Select which source should be used to determine whether the batteries are charged or discharged.")</script><br>
<script type="text/javascript">_dw("Default uses internal BACS method to determine battery discharge status.")</script>
</div>
<div class = "tt" id = "DischargeThreshold">
<script type="text/javascript">_dw("A discharge status is shown as a negative value in Ampere at the BACS CS current sensor status. To avoid false discharge alarms please set the level in Ampere you want to tolerate as discharge float for this setup. Enter a value to define the treshold for discharge status.")</script>
</div>
<div class = "tt" id = "ChargeThreshold">
<script type="text/javascript">_dw("A charge status is shown as a positive value in Ampere at the BACS CS current sensor status. To avoid false charge status LED please set the level in Ampere you want to tolerate as charge float for this setup. Enter a value to define the treshold for charge status.")</script>
</div>
<div class = "tt" id = "resetDischargeCtr">
<script type="text/javascript">_dw("Set the discharge counter back to Zero.")</script>
</div>
<div class="tt" id="bIsMetricSystemTTID">
<script type="text/javascript">_dw("Switch between Celsius and Fahrenheit scale for temperature.")</script><br>
<script type="text/javascript">_dw("For a change of this setting to take effect, a reboot or &quot;Restart BACS bus&quot; is required.")</script>
</div>

<div class = "tt" id = "trs">
<script type="text/javascript">_dw("Thermal runaway is defined as an increase of temperature at a higher input current than usual over a period of time.")</script>
</div>
<div class = "tt" id = "trs_temdiff">
<script type="text/javascript">_dw("Enter the deviation from the average battery temperature in Degree Celsius or Fahrenheit to define a &quot;Thermal Runaway Alarm&quot;.")</script><br>
<script type="text/javascript">_dw("Default is 20&deg; Celsius above the average temperature.")</script>
</div>

<div class = "tt" id = "trs_current">
<script type="text/javascript">_dw("Enter the input current in A at a &quot;Max. Module Temperature Difference&quot; to define a &quot;Thermal Runaway Alarm&quot;.")</script><br>
<script type="text/javascript">_dw("Default is 10 A higher than the average float charge current.")</script><br>
<script type="text/javascript">_dw("0.0 defines that this parameter is ignored and only the &quot;Max. Module Temperature Difference&quot; value determines the &quot;Thermal Runaway Alarm&quot;.")</script>
</div>

<div class = "tt" id = "trs_minutes">
<script type="text/javascript">_dw("Enter the time in Minutes the above 2 conditions (Max. Module Temperature Difference + Max. Current per String) have to be TRUE to trigger the &quot;Thermal Runaway Alarm&quot;.")</script><br>
<script type="text/javascript">_dw("Default is 30 minutes.")</script><br>
<script type="text/javascript">_dw("0.0 disables this option.")</script>
</div>
<div class = "tt" id = "trs_numraux">
<script type="text/javascript">_dw("Enter the number of GX_R_AUX devices in your BACS bus.")</script>
</div>

<div class = "tt" id = "trs_bbcfg">
<b><script type="text/javascript">_dw("Do not trip Battery-Breakers")</script>:</b><br>
<script type="text/javascript">_dw("This does not make use the predefinitions for Thermal Runaway.")</script><br>
<br>
<b><script type="text/javascript">_dw("Trip a single Battery-Breaker")</script>:</b><br>
<script type="text/javascript">_dw("This changes the GX_R_AUX Output 1 label to a new text &quot;%0&quot; and configures the event &quot;BACS Thermal Runaway Alarm&quot; to trip one Battery-Breaker for all Strings.",null,"Trip Battery-Breaker for All Strings")</script><br>
<br>
<b><script type="text/javascript">_dw("Trip separate Battery-Breakers for each string")</script>:</b><br>
<script type="text/javascript">_dw("This changes the GX_R_AUX Output 1 label to a new text &quot;%0&quot; (1-4) and configures the events &quot;BACS Thermal Runaway String x&quot; to trip one Battery-Breaker for each String.",null,"Trip Battery-Breaker String x")</script>
</div>

<div class = "tt" id = "csboxTT">
<b><script type="text/javascript">_dw("BACS CS Current Sensor Connected")</script>:</b><br>
<script type="text/javascript">_dw("Check this box if you have connected one or more current sensors to the BACS-Bus.")</script><br>
<i><script type="text/javascript">_dw("There can be only one current sensor active. Either via Sensorman over Com2 or the BACS Current Sensor.")</script></i>
</div>
<div class = "tt" id = "csmultTT">
<b><script type="text/javascript">_dw("Current Sensor Multiplier")</script>:</b><br>
<script type="text/javascript">_dw("Enter a multiplier for the current sensor values.")</script>
</div></div>
<div class = "tt" id = "csbox2TT">
<b><script type="text/javascript">_dw("Only One Current Sensor For All Strings")</script>:</b><br>
<script type="text/javascript">_dw("If you're going to use just one current sensor for all battery strings, check this box.")</script>
</div>
<div class = "tt" id = "csbox3TT">
<b><script type="text/javascript">_dw("Reverse Current Direction")</script>:</b><br>
<script type="text/javascript">_dw(" This option reverses the current sensor data for Discharge (-) and Charge (+) into the opposite. This function is useful if the current sensors have been mounted in the wrong direction.")</script>
</div>
