">

Analog Inputs |
--- | ---
Port | Name | Alarm (Low) | Alarm (High) | Sensor Range | Unit | Sensor Type
1 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
2 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
3 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
4 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
5 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
6 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
7 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
8 | " size=30 maxlength=31 class="ctrl"> | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> > | " size=6 maxlength=8 class="ctrl"> - " size=6 maxlength=8 class="ctrl"> | " size=8 maxlength=15 class="ctrl"> |
| Hysteresis: | " size=8 maxlength=5 class="ctrl">
| Lograte: | " size=8 maxlength=5 class="ctrl"> Seconds |

Digital Inputs |
--- | ---
Port | Name | NC Contact | Active | Port | Name | NC Contact | Active
1 | " size=30 maxlength=31 class="ctrl"> | > | > | 5 | " size=30 maxlength=31 class="ctrl"> | > | >
2 | " size=30 maxlength=31 class="ctrl"> | > | > | 6 | " size=30 maxlength=31 class="ctrl"> | > | >
3 | " size=30 maxlength=31 class="ctrl"> | > | > | 7 | " size=30 maxlength=31 class="ctrl"> | > | >
4 | " size=30 maxlength=31 class="ctrl"> | > | > | 8 | " size=30 maxlength=31 class="ctrl"> | > | >

Outlets |
--- | ---
Port | Name | PowerOn | Timer | Port | Name | PowerOn | Timer
1 | " size=30 maxlength=31 class="ctrl"> | > |  | 5 | " size=30 maxlength=31 class="ctrl"> | > |
2 | " size=30 maxlength=31 class="ctrl"> | > |  | 6 | " size=30 maxlength=31 class="ctrl"> | > |
3 | " size=30 maxlength=31 class="ctrl"> | > |  | 7 | " size=30 maxlength=31 class="ctrl"> | > |
4 | " size=30 maxlength=31 class="ctrl"> | > |  | 8 | " size=30 maxlength=31 class="ctrl"> | > |

Alarm Matrix |
--- | ---
Disable Outputs: > |

Sitemanger II Version: