# Help on 'SITEMANAGER'

Relais: This shows the actual status of Relais 1-8. These relais are normally connected with the power input of attached device, by changing the status of the Relais you can switch on/off these devices from remote. The SITEMANGER can manage up to 8 Relais. For more informations please see SITEMANAGER user manual.
Digital: This shows the current status of the Input/Output Port. This is a low voltage interface which can be set high or low. This interface may be used for Inputalarms (Smokedetector, Firealarm, Intruder Alarm, Aircondition Failure etc.) or as Outputalarm (Activation of external devices like Fire Extinguisher, etc.)
Analog: This shows the actual values of the analog devices (Temperature, Humidity sensors) in degree Celsius or percentage.
Green: This defines that this port is actually HIGH.
Red: This defines that this port is actually LOW.
Blue: This defines that this port is actually not active.
Yellow: This shows that this port is in an undefined status - Error.
For more information - see user manual of your CS121.