<div class="tt" id="aux">
When set as input in the configuration, this section will show either a picture of contact that is either closed (on) or open (off) indicating the status of an alarm that has been set in the configuration.<br><br>
When configured as output or a picture of a lightbulb on or off that has a button underneath it. This button can be set with administrator priviledges or can be left open for any user.
</div>
<div class="tt" id="ss4name">
Contains the user defined name for this Output.
</div>
<div class="tt" id="ss4img">
Indicates the current output status.<br><br>
<img src="/img/auxo0.gif" alt="" align="middle" width=45>&nbsp;:&nbsp;Output is low.<br><br>
<img src="/img/auxo1.gif" alt="" align="middle" width=45>&nbsp;:&nbsp;Output is high.
</div>
<div class="tt" id="ss4button">
Click on this button to toggle this output.<br>
(May require a password.)
</div>
<div class="tt" id="notempman">
Your can connect a &quot;Sensor Manager&quot; device to COM port 2.<br>
This device supports up to 8 analog sensors for monitoring temperature, humidity and other values.<br>
Click on the link below to get more informations about the Sensor Manager.
</div>
