">

Click YES to start a new BACS log file, that includes values from BACS current sensor. The current BACS log file will be deleted. All data that were logged today will be LOST! The new BACS log file will be started after reboot. To save this setting you must click the apply button and perform a 'Save, Exit and Reboot' cycle!

Click NO to keep all data that were logged today. Logging of data from the BACS current sensor will begin tomorrow. At the beginning of every day a new logfile with the current settings is started.

Click YES to start a new BACS log file, that excludes values from BACS current sensor. The current BACS log file will be deleted. All data that were logged today will be LOST! The new BACS log file will be started after reboot. To save this setting you must click the apply button and perform a 'Save, Exit and Reboot' cycle!

Click NO to keep all data that were logged today. Logging of data from the BACS current sensor will begin tomorrow. At the beginning of every day a new logfile with the current settings is started.

:
> | : |
> | : | " size = "6" maxlength = "5" class = "ctrl"> Ah
> | : | " size = "6" maxlength = "5" class = "ctrl"> > | : | " size = "6" maxlength = "5" class = "ctrl"> > | : | > > | : | /> />

:
> | : | " size="32" maxlength="63" class="ctrl"> > | : | " size="32" maxlength="63" class="ctrl"> > | : | " size="32" maxlength="63" class="ctrl"> > | : | " size="32" maxlength="63" class="ctrl"> > | : | " size="32" maxlength="63" class="ctrl"> > | : | " size="32" maxlength="63" class="ctrl">

1: | " size="32" maxlength="31"">
2: | " size="32" maxlength="31"">
3: | " size="32" maxlength="31"">
4: | " size="32" maxlength="31"">
5: | " size="32" maxlength="31"">
6: | " size="32" maxlength="31"">
7: | " size="32" maxlength="31"">
8: | " size="32" maxlength="31"">
9: | " size="32" maxlength="31"">
10: | " size="32" maxlength="31"">

> : | >
> : | > | >
: | >" size = "6" maxlength = "5" class = "ctrl"> V | >" size = "6" maxlength = "5" class = "ctrl"> V
: | >" size = "6" maxlength = "5" class = "ctrl"> °C | >" size = "6" maxlength = "5" class = "ctrl"> °C
> : | >" size = "6" maxlength = "5" class = "ctrl"> mΩ | >" size = "6" maxlength = "5" class = "ctrl"> mΩ
> > | > V
> : | > | >
: | >" size = "6" maxlength = "5" class = "ctrl"> V | >" size = "6" maxlength = "5" class = "ctrl"> V
: | V | V
: | >" size = "6" maxlength = "5" class = "ctrl"> °C | >" size = "6" maxlength = "5" class = "ctrl"> °C
> : | >" size = "6" maxlength = "5" class = "ctrl"> mΩ | >" size = "6" maxlength = "5" class = "ctrl"> mΩ
| > : | >
:
> | : | " size = "6" maxlength = "5" class = "ctrl"> °C
id = "tRowImpOffset"> | : | " size = "6" maxlength = "5" class = "ctrl"> mΩ
> | : | > > | : | > | : | > > | : | > > | : |
> | A
> | A
> | : |

> |
> : | " size="6" maxlength="5" class="ctrl"> °C
> | : | " size="6" maxlength="5" class="ctrl"> A > | : | " size="6" maxlength="5" class="ctrl">

> : > |

> |