">

Analog Inputs |
--- | ---
Port | Name | Threshold (Low) | Threshold (High) | Sensor Range (Low) | Sensor Range (High)
1 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
2 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
3 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
4 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
5 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
5 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
7 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
8 | " size=32 maxlength=31 class="ctrl"> | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> > | " size=8 maxlength=8 class="ctrl"> | " size=8 maxlength=8 class="ctrl">
| Hysteresis: | " size=8 maxlength=5 class="ctrl"> |

Digital Inputs |
--- | ---
Port | Name | NC Contact | Active | Port | Name | NC Contact | Active
1 | " size=32 maxlength=31 class="ctrl"> | > | > | 5 | " size=32 maxlength=31 class="ctrl"> | > | >
2 | " size=32 maxlength=31 class="ctrl"> | > | > | 6 | " size=32 maxlength=31 class="ctrl"> | > | >
3 | " size=32 maxlength=31 class="ctrl"> | > | > | 7 | " size=32 maxlength=31 class="ctrl"> | > | >
4 | " size=32 maxlength=31 class="ctrl"> | > | > | 8 | " size=32 maxlength=31 class="ctrl"> | > | >

Outlets |
--- | ---
Port | Name | PowerOn | Port | Name | PowerOn
1 | " size=32 maxlength=31 class="ctrl"> | > | 5 | " size=32 maxlength=31 class="ctrl"> | >
2 | " size=32 maxlength=31 class="ctrl"> | > | 6 | " size=32 maxlength=31 class="ctrl"> | >
3 | " size=32 maxlength=31 class="ctrl"> | > | 7 | " size=32 maxlength=31 class="ctrl"> | >
4 | " size=32 maxlength=31 class="ctrl"> | > | 8 | " size=32 maxlength=31 class="ctrl"> | >

Alarm Matrix |
--- | ---