<div class="tt" id="cfgnet_01">
<b><script type="text/javascript">_dw("MAC Address")</script></b><br>
<script type="text/javascript">_dw("Registered Media Access Control address.")</script>
</div>

<div class="tt" id="cfgnet_02">
<b><script type="text/javascript">_dw("Network Card Speed")</script></b><br>
<script type="text/javascript">_dw("Sets the communication speed of the CS121 adapter.")</script><br>
<script type="text/javascript">_dw("(Auto sensing option may result in temporary communication problems and delays when used with other auto sensing devices.)")</script>
</div>

<div class="tt" id="cfgnet_03">
<b><script type="text/javascript">_dw("Local Address")</script></b><br>
<script type="text/javascript">_dw("IP address that will be assigned to the adapter if DHCP is unused or failed.")</script>
</div>

<div class="tt" id="cfgnet_04">
<b><script type="text/javascript">_dw("Gateway Address")</script></b><br>
<script type="text/javascript">_dw("Address of the machine in local network segment for reaching other networks.")</script>
</div>

<div class="tt" id="cfgnet_05">
<b><script type="text/javascript">_dw("Subnet Mask")</script></b><br>
<script type="text/javascript">_dw("Defines the scope of local network segment for reducing network traffic.")</script>
</div>

<div class="tt" id="cfgnet_06">
<b><script type="text/javascript">_dw("Administrator Password")</script></b><br>
<script type="text/javascript">_dw("Password for FTP access, telnet access & administrator web pages.")</script><br><br>
<script type="text/javascript">_dw("All initial adapter passwords are set to 'cs121-snmp'. It is recommended that users immediately configure their own unique password to prevent unauthorised system access.")</script>
</div>

<div class="tt" id="cfgnet_07">
<b><script type="text/javascript">_dw("UNMS Server Password")</script></b><br>
<script type="text/javascript">_dw("Password for UNMS Server access and for switching AUX or SensorMan Outlets.")</script><br>
<script type="text/javascript">_dw("Leave blank to grant access to all users.")</script>
</div>

<div class="tt" id="cfgnet_08">
<b><script type="text/javascript">_dw("System Name")</script></b><br>
<script type="text/javascript">_dw("Description of system.")</script><br>
<script type="text/javascript">_dw("Will be used for administrator email subject.")</script>
</div>

<div class="tt" id="cfgnet_09">
<b><script type="text/javascript">_dw("System Location")</script></b><br>
<script type="text/javascript">_dw("Physical location of UPS location.")</script>
</div>

<div class="tt" id="cfgnet_10">
<b><script type="text/javascript">_dw("System Contact")</script></b><br>
<script type="text/javascript">_dw("Information about system administrator.")</script>
</div>

<div class="tt" id="cfgnet_11">
<b><script type="text/javascript">_dw("Attached Devices")</script></b><br>
<script type="text/javascript">_dw("Devices that are electrically connected to UPS.")</script>
</div>

<div class="tt" id="cfgnet_12">
<b><script type="text/javascript">_dw("Enable Telnet Server")</script></b><br>
<script type="text/javascript">_dw("Check box for enabling this functionality, if this box is not checked no telnet connection can be made to the adapter.")</script>
</div>

<div class="tt" id="cfgnet_13">
<b><script type="text/javascript">_dw("Enable HTTP Server")</script></b><br>
<script type="text/javascript">_dw("This enables the Webserver of the CS121.")</script><br><br>
<script type="text/javascript">_dw("Warning, if communication routes to the adapter are completely disabled, the adapter becomes a closed system and the only way to reconfigure and reestablish direct communications with the CS121 is to enact a full system setup.")</script>
</div>

<div class="tt" id="cfgnet_14">
<b><script type="text/javascript">_dw("Enable HTTP Tooltips")</script></b><br>
<script type="text/javascript">_dw("Uncheck to hide most tooltips in the CS121 web pages (like this one).")</script><br>
<script type="text/javascript">_dw("Unlike the other values on this page no reboot is necessary apply this.")</script>
</div>

<div class="tt" id="cfgnet_httpcache">
<b><script type="text/javascript">_dw("Enable HTTP Caching")</script></b><br>
<script type="text/javascript">_dw("Uncheck to disable the usage of the browser cache.")</script><br>
<script type="text/javascript">_dw("Unlike the other values on this page no reboot is necessary apply this.")</script>
</div>

<div class="tt" id="cfgnet_16">
<b><script type="text/javascript">_dw("Enable UNMS Server")</script></b><br>
<script type="text/javascript">_dw("When this option is enabled, the adapters information can be shown using UNMS, and will show up in the list of Upsman servers when UNMS does a server scan.")</script><br>
</div>

<div class="tt" id="cfgnet_17">
<b><script type="text/javascript">_dw("Use RCCMD2 Traps")</script></b><br>
<script type="text/javascript">_dw("This option is necessary to use the RCCMD trap event job.")</script>
</div>

<div class="tt" id="cfgnet_18">
<b><script type="text/javascript">_dw("Enable RCCMD Listener")</script></b><br>
<script type="text/javascript">_dw("Check this box to use the CS121 as an RCCMD client.")</script>
</div>

<div class="tt" id="cfgnet_19">
<b><script type="text/javascript">_dw("RCCMD Listener Port")</script></b><br>
<script type="text/javascript">_dw("Listen to this port when acting as RCCMD client.")</script><br>
<script type="text/javascript">_dw("Do not change this value without good reason!")</script>
</div>

<div class="tt" id="cfgnet_24">
<b><script type="text/javascript">_dw("Enable Modbus over IP")</script></b><br>
<script type="text/javascript">_dw("Enables the Modbus server.")</script>
</div>

<div class="tt" id="cfgnet_25">
<b><script type="text/javascript">_dw("Modbus Slave Address")</script></b><br>
<script type="text/javascript">_dw("The modbus slave address of the CS121 adapter.")</script>
</div>

<div class="tt" id="cfgnet_26">
<b><script type="text/javascript">_dw("Modbus Mode")</script></b><br>
<script type="text/javascript">_dw("The modbus slave and server mode must be matching for this function to perform properly.")</script>
</div>

<div class="tt" id="cfgnet_27">
<b><script type="text/javascript">_dw("RCCMD Timeout")</script></b><br>
<script type="text/javascript">_dw("Timeout for the RCCMD client in seconds.")</script>
</div>

<div class="tt" id="cfgnet_28">
<b><script type="text/javascript">_dw("UNMS Server Password for Web Pages")</script></b><br>
<script type="text/javascript">_dw("When enabled the CS121 uses the UNMS Server password for web access.")</script>
</div>

<div class="tt" id="cfgnet_30">
<b><script type="text/javascript">_dw("HTTP Port")</script></b><br>
<script type="text/javascript">_dw("The HTTP Port. Default: 80")</script>
</div>

<div class="tt" id="cfgnet_31">
<b><script type="text/javascript">_dw("HTTP Refresh Time")</script></b><br>
<script type="text/javascript">_dw("Main page refresh time in seconds.")</script>
</div>

<div class="tt" id="cfgnet_32">
<b><script type="text/javascript">_dw("HTTP Default Page")</script></b><br>
<script type="text/javascript">_dw("The page that will be shown when you connect to the CS121.")</script>
</div>

<div class="tt" id="cfgnet_33">
<b><script type="text/javascript">_dw("DNS Server")</script></b><br>
<script type="text/javascript">_dw("IP Address of the DNS server used by the CS121.")</script>
</div>

<div class="tt" id="cfgnet_40">
<b><script type="text/javascript">_dw("Enable LED Display Sender")</script></b><br>
<script type="text/javascript">_dw("Check this box to send UPS data to the LED Display.")</script>
</div>

<div class="tt" id="cfgnet_41">
<b><script type="text/javascript">_dw("LED Display Sender ID")</script></b><br>
<script type="text/javascript">_dw("Enter a unique id for this LED Display Sender, range is [0-9].")</script>
</div>

<div class="tt" id="cfgnet_42">
<b><script type="text/javascript">_dw("LED Display Listener Address")</script></b><br>
<script type="text/javascript">_dw("Enter the IP address of the LED Display in local network segment.")</script>
</div>

<div class="tt" id="cfgnet_43">
<b><script type="text/javascript">_dw("LED Display Listener Timeout")</script></b><br>
<script type="text/javascript">_dw("Enter the timeout in seconds for keeping last sent LED Display values.")</script>
</div>

<div class="tt" id="cfgnet_51">
<b><script type="text/javascript">_dw("Static ARP Entries")</script></b><br>
<script type="text/javascript">_dw("Set answer IP address for network cards using HP teaming and load balancing.")</script>
</div>

<div class="tt" id="cfgnet_rccmdssl">
<b><script type="text/javascript">_dw("Use RCCMD SSL")</script></b><br>
<script type="text/javascript">_dw("Use SSL encryption when sending RCCMD commands.")</script><br>
<i><script type="text/javascript">_dw("Using a timeserver is required when using this option!")</script></i>
</div>

<div class="tt" id="cfgnet_dhcp">
<b><script type="text/javascript">_dw("Use DHCP")</script></b><br>
<script type="text/javascript">_dw("Receive IP address from DHCP server.")</script><br>
<script type="text/javascript">_dw("You can configure a specific DHCP server or use 255.255.255.255 for DHCP broadcast.")</script>
</div>

<div class="tt" id="cfgnet_upsmonport">
<b><script type="text/javascript">_dw("UNMS Port")</script></b><br>
<script type="text/javascript">_dw("The UNMS Port. Default: 5769")</script>
</div>

<div class="tt" id="cfgnet_hidelink3">
<b><script type="text/javascript">_dw("Hide HTTP Device Functions Link")</script></b><br>
<script type="text/javascript">_dw("Hide the link to the Device Functions page in the main menu on the left side.")</script>
</div>

<div class="tt" id="cfgnet_use_icmp">
<b><script type="text/javascript">_dw("Use ICMP Check")</script></b><br>
<script type="text/javascript">_dw("Mark this checkbox and enter up to 3 IP addresses to enable the ICMP check.")</script><br>
<script type="text/javascript">_dw("This will periodically send a Ping to the configured addresses to check the state of the CS121 TCP/IP stack.")</script><br>
<i><script type="text/javascript">_dw("It is recommended to use the Gateway address here.")</script></i>
</div>

<div class="tt" id="cfgnet_useftp">
<b><script type="text/javascript">_dw("Enable FTP Server")</script></b><br>
<script type="text/javascript">_dw("Check box for enabling this functionality, if this box is not checked no FTP connection can be made to the adapter.")</script><br>
<script type="text/javascript">_dw("It is not recommended to disable the FTP server.")</script>
</div>

<div class="tt" id="cfgnet_serviceport">
<b><script type="text/javascript">_dw("Service & Update Port")</script></b><br>
<script type="text/javascript">_dw("This port is used for firmware update.")</script><br>
<script type="text/javascript">_dw("Setting this port to 0 will disable the firmware update.")</script><br>
<b><script type="text/javascript">_dw("This is not recommended!")</script></b>
</div>

<div class="tt" id="cfgnet_gsmip">
<b><script type="text/javascript">_dw("RASMAN_G IP Address")</script></b><br>
<script type="text/javascript">_dw("Rasmanager GSM IP address.")</script><br>
<script type="text/javascript">_dw("Enter 0.0.0.0 to disable.")</script>
</div>

<div class="tt" id="cfgnet_gsmport">
<b><script type="text/javascript">_dw("RASMAN_G IP Port")</script></b><br>
<script type="text/javascript">_dw("Rasmanager GSM IP Port")</script><br>
<script type="text/javascript">_dw("Default")</script> 6000
</div>

<div class="tt" id="cfgnet_tcpmss">
<b><script type="text/javascript">_dw("TCP MSS")</script></b><br>
<script type="text/javascript">_dw("TCP Maximum Segment Size.")</script><br>
<script type="text/javascript">_dw("Default")</script> 1460
</div>

<div class="tt" id="cfgnet_hostname">
<b><script type="text/javascript">_dw("Hostname")</script></b><br>
<script type="text/javascript">_dw("Prefered hostname when using DHCP")</script>
</div>

<div class="tt" id="cfgnet_forcegateway">
<b><script type="text/javascript">_dw("Force configured Gateway")</script></b><br>
<script type="text/javascript">_dw("Enable to force all answers through the configured gateway.")</script><br>
<script type="text/javascript">_dw("Disable (default) to answer all answers directly to requesting IP address.")</script>
</div>

<div class="tt" id="cfgnet_https">
<b><script type="text/javascript">_dw("Use HTTPS")</script></b><br>
<script type="text/javascript">_dw("This enables HTTPS. Normal HTTP will be disabled.")</script><br>
</div>

<div class="tt" id="cfgnet_httpsport">
<b><script type="text/javascript">_dw("HTTPS Port")</script></b><br>
<script type="text/javascript">_dw("The HTTPS Port. Default: 443")</script>
</div>

<div class="tt" id="cfgnet_savelog">
<b><script type="text/javascript">_dw("Save Logfiles automatically")</script></b><br>
<script type="text/javascript">_dw("Backup logfiles to flash disk every 24 hours.")</script><br>
<script type="text/javascript">_dw("This may cause a delay for some network services.")</script>
</div>

<div class="tt" id="cfgnet_arpcache">
<b><script type="text/javascript">_dw("Auto-Update ARP Cache")</script></b><br>
<script type="text/javascript">_dw("If enabled static ARP will be be changed to &quot;Gratuitous ARP request&quot;")</script>
</div>
