<div class="tt" id="cfgmodel_01">
<b><script type="text/javascript">_dw("UPS Model")</script></b><br>
<script type="text/javascript">_dw("Dropdown selection of available UPS models (contact manufacturer or support for non listed models).")</script><br>
<script type="text/javascript">_dw("Default values for power, load, hold time, recharge time, baud rate, and cable type are automatically according to the selected model. Changing of these values may result in UPS communication malfunctioning.")</script>
</div>

<div class="tt" id="cfgmodel_02">
<b><script type="text/javascript">_dw("Power")</script></b><br>
<script type="text/javascript">_dw("UPS nominal power in VA.")</script>
</div>

<div class="tt" id="cfgmodel_03">
<b><script type="text/javascript">_dw("Load")</script></b><br>
<script type="text/javascript">_dw("Actual UPS load in VA.")</script>
</div>

<div class="tt" id="cfgmodel_04">
<b><script type="text/javascript">_dw("Hold Time")</script></b><br>
<script type="text/javascript">_dw("Time in minutes that the battery can sustain the specified load.")</script>
</div>

<div class="tt" id="cfgmodel_05">
<b><script type="text/javascript">_dw("Recharge Time")</script></b><br>
<script type="text/javascript">_dw("Time in hours for recharging the battery to full capacity after a complete discharge.")</script>
</div>

<div class="tt" id="cfgmodel_06">
<b><script type="text/javascript">_dw("Baud Rate")</script></b><br>
<script type="text/javascript">_dw("Serial communication speed for the selected UPS model.")</script>
</div>

<div class="tt" id="cfgmodel_07">
<b><script type="text/javascript">_dw("Cable Type")</script></b><br>
<script type="text/javascript">_dw("Specifies the type of cable used for connecting the CS121 adapter and UPS together.")</script>
</div>

<div class="tt" id="cfgmodel_08">
<b><script type="text/javascript">_dw("Exchange COM Ports")</script></b><br>
<script type="text/javascript">_dw("Check box for switching COM1 and COM2 on the CS121 adapter for enabling alternative cable connections.")</script>
</div>

<div class="tt" id="cfgmodel_09">
<b><script type="text/javascript">_dw("UPS ID")</script></b><br>
<script type="text/javascript">_dw("Only for modular UPS!")</script><br>
<script type="text/javascript">_dw("For single UPS please enter UPS ID of your UPS module configuration, for single UPS usually '1'. '0' defines to talk to all modules in the bus via the MULTIDROP slot of the UPS. UPS ID's are supported as positive integer values from 1 to 15. Exception: An UPS ID as '1-' switches to a previous protocol of older modular UPS.")</script>
</div>

<div class="tt" id="cfgmodel_10">
<b><script type="text/javascript">_dw("System Name")</script></b><br>
<script type="text/javascript">_dw("Description of system.")</script><br>
<script type="text/javascript">_dw("Will be used for administrator email subject.")</script>
</div>

<div class="tt" id="cfgmodel_11">
<b><script type="text/javascript">_dw("System Location")</script></b><br>
<script type="text/javascript">_dw("Physical description of UPS location.")</script>
</div>

<div class="tt" id="cfgmodel_12">
<b><script type="text/javascript">_dw("System Contact")</script></b><br>
<script type="text/javascript">_dw("Information about system administrator.")</script>
</div>

<div class="tt" id="cfgmodel_13">
<b><script type="text/javascript">_dw("Attached Devices")</script></b><br>
<script type="text/javascript">_dw("Devices that are electrically connected to UPS.")</script>
</div>

<div class="tt" id="cfgmodel_14">
<b><script type="text/javascript">_dw("Battery Installation Date")</script></b><br>
<script type="text/javascript">_dw("Firmware update defaults to date of update and user must set the real date of UPS installation.")</script>
</div>

<div class="tt" id="cfgmodel_15">
<b><script type="text/javascript">_dw("Custom Values")</script></b><br>
<script type="text/javascript">_dw("These variables could be used to build special UPSMON screens, web pages, logfile entries and so on.")</script>
</div>

<div class="tt" id="cfgmodel_17">
<b><script type="text/javascript">_dw("System Shutdown Time")</script></b><br>
<script type="text/javascript">_dw("Enter the time in minutes you want CS121 to start the event 'System Shutdown'.")</script><br>
<script type="text/javascript">_dw("Default is close to UPS battery end - 3 minutes. This will start the shutdown only if the UPS has been discharged to a level of just 3 minutes left. Be sure that the default of 3 minutes is enough to send and finish you RCCMD shutdown commands, otherwise change this value accordingly.")</script>
</div>

<div class="tt" id="cfgmodel_pt2slave">
<b><script type="text/javascript">_dw("PipeThrough Slave")</script></b><br>
<script type="text/javascript">_dw("This increases timeouts for some UPS models.")</script>
</div>
