<div class="tt" id="cfgras_01">
<b>Modem</b><br>Select your modem type here.
</div>
<div class="tt" id="cfgras_02">
<b>License Key</b><br>This is the key code that was delivered with you RASManager, RASManager modem, or RASControl software.
</div>
<div class="tt" id="cfgras_03">
<b>Modem Init String</b><br>This is a value that is automatically set for the supported modems. Although other modems work with the CS121 series RAS function no support is provided for setting the Init strings of non-supported modems.
</div>
<div class="tt" id="cfgras_04">
<b>Modem First Time Init</b><br>This is a value that is automatically set for the supported modems. Although other modems work with the CS121 series RAS function no support is provided for setting the Init strings of non-supported modems.
</div>
<div class="tt" id="cfgras_05">
<b>RAS Manager Phone Number</b><br>This is just a spot to note down the telephone number of RASManager for reference.
</div>
<div class="tt" id="cfgras_06">
<b>Act as Client</b><br>Setting this check box will enable the adapter to make dial-up connections to the designated machine in the Destination IP Address.
</div>
<div class="tt" id="cfgras_07">
<b>Operation Timeout</b><br>This is the amount of seconds the adapter will attempt to establish a dial-up connection per attempt.
</div>
<div class="tt" id="cfgras_08">
<b>Number to Dial</b><br>This is the telephone number of the machine the RAS Manager will call.
</div>
<div class="tt" id="cfgras_09">
<b>Number of Connection Attempts</b><br>This is the number of times the RAS Manager will attempt to establish a dial-up connection before giving up if no connection can be made.
</div>
<div class="tt" id="cfgras_10">
<b>Destination Address</b><br>This is the IP address of the machine being called.
</div>
<div class="tt" id="cfgras_11">
<b>Username</b><br>This is the account name the RAS Manager will use as client.
</div>
<div class="tt" id="cfgras_12">
<b>Password</b><br>This is the user password for the RAS Managers user account.
</div>
<div class="tt" id="cfgras_13">
<b>Confirm Password</b><br>This is a safe check on the correct entry of the password.
</div>
<div class="tt" id="cfgras_14">
<b>Inactivity Timeout</b><br>This is the number of seconds after which the RAS Manager will disconnect the incoming connection when no communications have been registered.
</div>
<div class="tt" id="cfgras_15">
<b>Act as Server</b><br>Setting this check box will enable the RAS Manager to register and answer incoming calls..
</div>
<div class="tt" id="cfgras_16">
<b>Enable Callback</b><br>This places a condition on the Act as Server mode that allow the RASManager to register incoming calls, but cause the RASManager to call back the machine designated in the Act as Client section and not to answer the call.
</div>
<div class="tt" id="cfgras_17">
<b>Server IP Address</b><br>This is the IP Address that the RASManager will use when acting as server.
</div>
<div class="tt" id="cfgras_18">
<b>Username</b><br>same as in the act as client section but for the server mode.
</div>
<div class="tt" id="cfgras_19">
<b>Password</b><br>same as in the act as client section but for the server mode.
</div>
<div class="tt" id="cfgras_20">
<b>Confirm Password</b><br>same as in the act as client section but for the server mode.
</div>