# Help on 'Network Status'

MAC Adress: MAC Adress of your CS 121 device.
Network Speed: UNITS Mbit. Actual settings of your Ethernet card inside CS121. 10half, 10full, 100half, 100full or AUTOSENSING
IP Adress: TCP IP Adress of your CS121.
Subnet Mask: Subnetmask of your CS121.
Default Gateway: Gateway IP Adress of your CS121.
Email Server: SMTP Email Server of your CS121, IP Adress is required ! Do not use hostname.
Telnet Server: Actual status of your TELNET Server inside CS121. On/Off.
HTTP Server: Actual status of your Webbrowser Server inside CS121. On/Off.
SNMP Server: Actual status of your SNMP Server inside CS121. On/Off.
Upsmon Server: Actual status of your UPSMAN UPSTCP Server inside CS121. On/Off.
Use SNMP Coldboot Trap: If enabled, the CS121 sends an SNMP Trap to your NMS Station. Default is OFF. On/Off.
Use SNMP Authentication Trap: If enabled, the CS121 sends a Warning SNMP Trap to your NMS Station if any user tries to request data from your CS121 without having rights (defined in ACCESS Controls). Default is OFF. On/Off.
For more information - see user manual of your CS121.