">

BACS Settings 1 (These values require a reboot to become active) |
--- | ---
Module Type: |
Battery Capacity: | " size=4 maxlength=3 class="ctrl"> Ah
Log Rate (Normal Operation): | " size=4 maxlength=5 class="ctrl"> Seconds
Log Rate (Charge/Discharge): | " size=4 maxlength=5 class="ctrl"> Seconds
Number of Battery Modules: | " size=4 maxlength=3 class="ctrl">
Number of Battery Strings: | " size=4 maxlength=3 class="ctrl">
Warn if size of CompactFlash less than: (Currenty of KB free) | " size=4 maxlength=6 class="ctrl"> KB

BACS Settings 2 (These values will become active immediately) |
--- | ---
Battery Alarm Level: | " size=4 maxlength=4 class="ctrl"> mΩ
Battery Warning Level: | " size=4 maxlength=4 class="ctrl"> mΩ
Temp. Alarm below: | " size=4 maxlength=3 class="ctrl"> °C
Temp. Alarm above: | " size=4 maxlength=3 class="ctrl"> °C
Volt. Alarm below: | " size=4 maxlength=4 class="ctrl"> V
Volt. Alarm above: | " size=4 maxlength=4 class="ctrl"> V
Pollrate Internal Resistance: | " size=4 maxlength=3 class="ctrl"> minutes
Voltage Range for Internal Resistance Polling: | " size=4 maxlength=4 class="ctrl"> - " size=4 maxlength=4 class="ctrl"> V
Use Buzzer: | >

Error Mask (Marked events will not generate error messages or warnings) |
--- | ---
Module | System | Voltage | Temperature | Resistance |
Auto-Reset Alarms:
System: > Voltage: > Temperature: > Resistance Warning: > Resistance Alarm: >