<div class="tt" id="network_01">
<b>MAC Address</b><br>Registered Media Access Control number.
</div>
<div class="tt" id="network_02">
<b>Network Speed</b><br>Ethernet communication speed of the CS121 adapter.
</div>
<div class="tt" id="network_03">
<b>IP Address</b><br>Default IP address that will assigned to the adapter unless DHCP is active.
</div>
<div class="tt" id="network_04">
<b>Subnet Mask</b><br>Defines the scope of local network segment for reducing network traffic.
</div>
<div class="tt" id="network_05">
<b>Default Gateway</b><br>Address of the machine in local network segment for reaching other networks.
</div>
<div class="tt" id="network_06">
<b>EMail Server</b><br>Hostname or IP address of the mail server.
</div>
<div class="tt" id="network_07">
<b>Time Server</b><br>IP address of the server that the CS121 uses for setting its clock.
</div>
<div class="tt" id="network_08">
<b>Telnet Server</b><br>Indicates whether the CS121 telnet server is running or not.
</div>
<div class="tt" id="network_09">
<b>HTTP Server</b><br>Indicates whether the CS121 web server is running or not.<br>Obviously it is. <img src="/img/smile.gif" alt=":)" border=0>
</div>
<div class="tt" id="network_10">
<b>Upsmon Server</b><br>Indicates whether the CS121 UPSMON server is running or not.<br><br>
When this option is enabled, the adapters information can be shown using UPSMON, and will show up in the list of Upsman servers when UPSMON does a server scan.
</div>
<div class="tt" id="network_11">
<b>Use RCCMD2 Traps</b><br>Indicates whether the CS121 supports RCCMD traps or not.<br>
This is necessary to use the RCCMD trap event job.
</div>
<div class="tt" id="network_12">
<b>SNMP Server</b><br>Indicates whether the CS121 SNMP agent feature is activated or not.
</div>
<div class="tt" id="network_13">
<b>Use SNMP Coldboot Trap</b><br>Indicates whether the CS121 sends a SNMP coldboot trap on startup or not.
</div>
<div class="tt" id="network_14">
<b>Use SNMP Authentication Trap</b><br>Indicates whether the CS121 sends a SNMP authentication trap on SNMP access violations or not.
</div>
<div class="tt" id="network_15">
<b>Modbus Server</b><br>Indicates whether the CS121 modbus over IP feature is activated or not.
</div>
<div class="tt" id="network_16">
<b>DNS Server</b><br>IP address of the used DNS server.
</div>
