<div class="tt" id="cfgmodel_01">
<b>UPS Model</b><br>
Dropdown selection of available UPS models (contact manufacturer or support for non listed models).<br>
Default values for power, load, hold time, recharge time, baud rate, and cable type are automatically according to the selected model. Changing of these values may result in UPS communication malfunctioning.
</div>
<div class="tt" id="cfgmodel_02">
<b>Power</b><br>UPS nominal power in VA.
</div>
<div class="tt" id="cfgmodel_03">
<b>Load</b><br>Actual UPS loadn in VA.
</div>
<div class="tt" id="cfgmodel_04">
<b>Hold Time</b><br>Time in minutes that the battery can sustain the specified load.
</div>
<div class="tt" id="cfgmodel_05">
<b>Recharge Time</b><br>Time in hours for recharging the battery to full capacity after a complete discharge.
</div>
<div class="tt" id="cfgmodel_06">
<b>Baud Rate</b><br>Serial communication speed for the selected UPS model.
</div>
<div class="tt" id="cfgmodel_07">
<b>Cable Type</b><br>Specifies the type of cable used for connecting the CS121 adapter and UPS together.
</div>
<div class="tt" id="cfgmodel_08">
<b>Exchange COM Ports</b><br>Check box for switching COM1 and COM2 on the CS121 adapter for enabling alternative cable connections.
</div>
<div class="tt" id="cfgmodel_09">
<b>UPS ID</b><br>
Only for modular UPS!<br>
For single UPS please enter UPS ID of your UPS module configuration, for single UPS usually "1".
"0" defines to talk to all modules in the bus via the MULTIDROP slot of the UPS.
UPS ID's are supported as positive integer values from 1 to 15.
Exception: An UPS ID as "1-" switches to a previous protocol of older modular UPS.
</div>
<div class="tt" id="cfgmodel_10">
<b>System Name</b><br>Description of system.<br>Will be used for administrator email subject.
</div>
<div class="tt" id="cfgmodel_11">
<b>System Location</b><br>Physical description of UPS location.
</div>
<div class="tt" id="cfgmodel_12">
<b>System Contact</b><br>Information about system administrator.
</div>
<div class="tt" id="cfgmodel_13">
<b>Attached Devices</b><br>Devices that are electrically connected to UPS.
</div>
<div class="tt" id="cfgmodel_14">
<b>Battery Installation Date</b><br>Firmware update defaults to date of update and user must set the real date of UPS installation.
</div>
<div class="tt" id="cfgmodel_15">
<b>Custom Values</b><br>These variables could be used to build special UPSMON screens, web pages, logfile entries and so on.
</div>
<div class="tt" id="cfgmodel_17">
<b>System Shutdown Time</b><br>
Enter the time in minutes you want CS121 to start the event &quot;System Shutdown&quot;.<br>
Default is close to UPS battery end - 3 minutes. Thsis will start the shutdown only if the UPS has been discharged to a level of just 3 minutes left.
Be sure that the default of 3 minutes is enough to send and finish you RCCMD shutdown commands, otherwise change this value accordingly.
</div>
