<div class="tt" id="bacs_volt_hdr">
This column shows the voltage of each module.
</div>
<div class="tt" id="bacs_temp_hdr">
This column shows the temperature of each module.
</div>
<div class="tt" id="bacs_resist_hdr">
This column shows the internal resistance (impedance) of each module.
</div>
<div class="tt" id="bacs_bp_hdr">
This column shows the bypass state of each module.<br>
<table style="font-family:verdana,arial,helvetica; font-size:11px;">
<tr><td><span class="grbar">&nbsp;&nbsp;&nbsp;</span> - Bypass less then 50 %</td></tr>
<tr><td><span class="gbar">&nbsp;&nbsp;&nbsp;</span> - Bypass 50 % or more</td></tr>
<tr><td><span class="rbar">&nbsp;&nbsp;&nbsp;</span> - Module data not available</td></tr>
</table>
Move the mouse cursor over the table rows to see exact bypass value.<br>
Bypass signals that equalizing is in progress.<br>
</div>
<div class="tt" id="bacs_state_hdr">
This column shows the alarm state of each module.<br>
Possible alarms:
<ul>
<li><b>System alarm:</b> indicates a problem with the BACS wiring or a bad BACS configuration.</li>
<li><b>Voltage alarm:</b> indicates that the voltage of this module is out of the configurated range.</li>
<li><b>Temperature alarm:</b> indicates that the temperature is out of the configurated range.</li>
<li><b>Resistance alarm:</b> indicates that the resistance is above the alarm level.<br>This battery should be replaced as soon as possible!</li>
<li><b>Resistance warning:</b> indicates that the resistance is above the warning level.</li>
</ul>
<i>Please note: All Alarms will be displayed until they are confirmed on the BACS module.</i>
</div>
