<div class="tt" id="upsstat_01">
<b>Status</b><br>Indicates the general status of the UPS: OK, on battery, bypass, and more.
</div>
<div class="tt" id="upsstat_02">
<b>Input Voltage</b><br>Current level of voltage input.
</div>
<div class="tt" id="upsstat_03">
<b>Input Frequency</b><br>Current frequency of input.
</div>
<div class="tt" id="upsstat_04">
<b>Output Voltage</b><br>Current level of UPS output voltage.
</div>
<div class="tt" id="upsstat_05">
<b>Output Frequency</b><br>Current frequency of output.
</div>
<div class="tt" id="upsstat_06">
<b>Load</b><br>Current load in percent in terms of UPS power.
</div>
<div class="tt" id="upsstat_07">
<b>Seconds on Battery</b><br>System counter in seconds during the &quot;on battery&quot; status.
</div>
<div class="tt" id="upsstat_08">
<b>Battery Voltage</b><br>Current UPS battery voltage.
</div>
<div class="tt" id="upsstat_09">
<b>Battery Capacity</b><br>Charge level of UPS battery in percent.
</div>
<div class="tt" id="upsstat_10">
<b>Autonomy Time</b><br>Calculated estimate of time remaining under the current load after which battery capacity will be exhausted.
</div>
<div class="tt" id="upsstat_11">
<b>Battery Temperature</b><br>Current temperature of UPS battery.
</div>
<div class="tt" id="loadbar">
This is both a graphical and numerical display of the current UPS load in percent of total available capacity.
</div>
<div class="tt" id="bcbar">
This is both a graphical and numerical display of the current UPS battery level in percent of total charging capacity.
</div>
